Home > Versión Plus > Funciones de Pago > Dispositivos Soportados > Lector billetes Smiley

Lector de Billetes Smiley NV4/7/8/9/10

El dispositivo de pago Smiley NV4/7/8/9/10 es un lector de billete que fue diseñado para proveedores de terminales de acceso público a Internet para cargar a los usuarios por el uso mediante billetes.
Esta compañía nos ha informado que sus dispositivos están funcionando correctamente utilizando el conjunto de cables RS232 adecuados. Los NV's se pueden utilizar con los tipos de moneda más utilizados en todo el mundo. Si tiene problemas con el hardware, por favor contacte a su fabricante o Innovative Technology. PROVISIO no vende este producto y no podrá ayudarle.
Nota:
Los lectores de bille Smiley son accesibles con el protocolo ccTalk Protocol que proporciona un mejor control que el simple protocolo Serie I/O. Por tanto le recomendamos utilizar el protocolo ccTalk. Si necesita cambiar la versión de firmware de su lector, el Fabricante le proporciona herramientas para ello.
1. Requisitos de Sistema
1.1 Hardware

1. Smiley NV4/7/8/9/10 bill acceptor
2. RS232 (COM) interface cable
   Protocol: Simple Serial Input/Output. Note: SSP - Smiley Secure Protocol is not supported
   NOTE:
   It is recommended to use the Smiley as a ccTalk device instead of using the Simple Serial Input/Output protocol.
3. 12 Volt PSU
4. Up-to-date PC with available COM port

1.2 Software

1. Windows 7, 8, 10
2. Internet Explorer 10, 11
3. SiteKiosk Plus License

2. Instalación de Hardware
2.1 Connect the cable to the computer
Plug the included COM port cable directly into the COM port of your computer.
2.2 Connect the cable to the bill acceptor
The other end of the cable is connected to the Smiley NV-housing. Make sure that the plug is connected correctly.
2.3 Power Supply
The Smiley NV requires a separate power supply and is normally included with the device. Plug the device into the appropriate connector on the COM-port cable. Make sure to pay attention to the polarity.
3. Configuración Smiley
3.1 General
After installing SiteKiosk and connecting the payment device to your computer, you can now configure the device using the SiteKiosk configuration tool. Select the entry Bill Acceptor: Smiley NV4/7/8/9/10 from the list of available devices then click the Customize button to configure and activate the device.
The icon next to the device will turn from red to green after the device has been activated.
3.2 Automatic Detection
Click on the button labeled Search. The Payment Module usually automatically detects which COM port you connected the Smiley to. If it should fail to do so, please check whether you have connected everything correctly and if the Smiley is powered on. If you are still not able to detect the device in SiteKiosk, please contact us .
3.3 Bill Values
After the device is recognized, activate all channels for the bills that you want to accept. After that, select your desired bill from the drop-down menu next to each channel. Next you can specify the money value of the bills displayed in relation to the main currency. Money value means that you can define the value of foreign currencies in relation to the main currency. However, as a rule, you should specify that the main currency is the same as the currency you can select here. Exit the window by clicking OK.

The device is now ready for use.
Edit SmileyNV4.ini:
If the currency you want to use is not available for selection you can add it by editing the file ..\SiteKiosk\SiteCash\SmileyNV4.ini. Open the file with an editor like Notepad and add new entries for your currency to the end of the existing list.

4. Solución de problemas
4.1 Bills are not being recognized
Make sure you selected the corresponding bill while you were configuring the Smiley.
4.2 Geldscheine werden nicht eingezogen

1. Check if the PSU is connected
2. Check the device for obstructions

Vea también

Diálogo Virtual de Simulación (para pruebas)
Sel. Monedas WH EMP800 y 850/Gest. cambio GW200/Escrow E104
Sel. Monedas Microcoin QL/Comex CX-363CA
Sel. Monedas (Pulsos)
Tarjetas de Crédito
SiteCafe para Cibercafés
Limitador de Tiempo
Interfaz ccTalk (varios)
Interfaz CCT900
Interfaz CoinRS (COM-Port)
Interfaz HW200 USB
PcCredit Board (COM-Port)
Lector billetes (varios)
Lector billetes CashCode
Lector billetes MEI EBDS

Volver arriba